README
======

  This is a test of the SMART file system that derives from
  testing/nxffs.

  * CONFIG_TESTING_SMART: - Enable the SMART file system example
  * CONFIG_TESTING_SMART_ARCHINIT: The default is to use the RAM MTD
    device at drivers/mtd/rammtd.c.  But an architecture-specific MTD
    driver can be used instead by defining CONFIG_TESTING_SMART_ARCHINIT.  In
    this case, the initialization logic will call smart_archinitialize()
    to obtain the MTD driver instance.
  * CONFIG_TESTING_SMART_NEBLOCKS: When CONFIG_TESTING_SMART_ARCHINIT is not
    defined, this test will use the RAM MTD device at drivers/mtd/rammtd.c
    to simulate FLASH.  In this case, this value must be provided to give
    the nubmer of erase blocks in MTD RAM device.  The size of the allocated
    RAM drive will be: CONFIG_RAMMTD_ERASESIZE * CONFIG_TESTING_SMART_NEBLOCKS
  * CONFIG_TESTING_SMART_MAXNAME: Determines the maximum size of names used
    in the filesystem
  * CONFIG_TESTING_SMART_MAXFILE: Determines the maximum size of a file
  * CONFIG_TESTING_SMART_MAXIO: Max I/O, default 347.
  * CONFIG_TESTING_SMART_MAXOPEN: Max open files.
  * CONFIG_TESTING_SMART_MOUNTPT: SMART mountpoint
  * CONFIG_TESTING_SMART_NLOOPS: Number of test loops. default 100
  * CONFIG_TESTING_SMART_VERBOSE: Verbose output
